|  |  |  |  |
| --- | --- | --- | --- |
|  | 3v3 | 5V | Platine 5V |
| Display | 8 | 5V |  |
| Display | 9 | GND |  |
|  | 7 | 15 |  |
| Platine GND | GND | 16 | RC2 |
| LED\_B | 0 | 1 | PWM |
| LED\_G | 2 | GND |  |
| LED\_R | 3 | 4 | RC3 |
|  | 3v3 | 5 |  |
| MOSI | 12 | GND | RC1 |
| MISO | 13 | 6 | DHT22 Data Pin |
| CLK | 14 | 10 | CS |
| Levelshifter GND | GND | 11 |  |

Using wiringPi numbering!

RC stands for relay channel